**The Comedy Store**

**Venue Technical Specifications**

An amphitheater style auditorium with seating for 400 people.

**Stage**

Steel Deck 12 x 8 ft minus 4ft radial curves on front corners

Expandable to 16 x 10 ft and various other configurations

1ft legs as standard

Black, pleated tabs on back wall (removable)

**Lighting**

- Power

3 Phase 63amp into Smartrack Dimmers with additional (in-line) 63amp 3 phase outlet

72 channels of DMX controlled dimming in 16amp outlets on internally wired bars (distribution shown in autocad file).

- Control

Avolites Pearl Expert

- Fixtures (moving)

Martin MAC250 Kryptons x 4

- Fixtures (generic)

Source 4 Parcans x 4

Source 4 Parnels x 6

Source 4 Zoom profiles x 2

Source 4 Junior profiles x 4

Strand 300w fresnels x 2

Strand 28/40 profiles x 4

Crown shortcan/floorcans Parcans (Silver) x 6

Thomas shortcan Parcans (Silver) x 2

Altmann 20 cell MR16 battens x 2

Jem 24/7 Hazer x 2

**Sound**

24 way multicore between Stage and control room

8 channel extension snake

- Control

Allen & Heath GLD 112 Digital Mixer

2 x Allen & Heath IDR-8

DT150 Headphones

- Main output

18 x HK Audio CT108

2 x HK Audio CDR210C Subs

7x HK Audio VX2400 Amplifiers

1 x LS400 Nexo sub

- Fold Back

4 x PS8 Nexo fold back wedges (2 flown, 2 floor mounted)

2 x Nexo PS8 Controller (Analogue)

Induction Loop for the hard of hearing covering one large area of seating

- Mics

SM58 x 6

Nueman KMS105 x 2

AKG C1000 Instrument mics x 2

Senheiser E614 x 4 (3 as audience mics)

Audio Technica AT4040 x 3 (as Audience mics)

Sennheiser SKM100-835 G3 hand held radio mic

G3 SK2000 radio mic receivers and body packs x 8

Sennheiser MKE2 Tie Clip radio mics x 2

6 x Audio Technica headset mics (terminated to SK2000)

3 x LA Audio active DI boxes

- Playback

Denon DN-D4500 CD/MP3 Player

Dualcore Power Mac

**Main Projector**

Christie LWU505 LCD Projector, 5000 Lumens, WXGA (HD), 1.7-2.8:1 Lens

Christie 0.8:1 Short Throw Fixed Lens Option

**Main Screen**

Option 1 – fully portable, Draper 16:9 HD Ultimate Fast Folding Screen. Front and back projection options: 2.44m x 1.42m

Option 2 – fixed at side of the stage, Duronic 16:9 electronic HD Projector Screen: 2.64m x 1.47m

**Second Screen Projection (servicing raised seating area)**

BenQ MW523 WXGA 3000 Lumens DLP Projector

Duronic 16:9  Manual Pull Down HD Projector Screen 2.21m x 1.25m

**Control**

Extron Matrix 8×8

Extron Switcher/scaler

VGA input points from control and stage positions to matrix

2 x Sony 250Gb Hard Disc/DVD recorder

2 x 56″ Plasma Screens for overspill viewing in bar area

**Dressing Room**

There is one dressing room backstage with a door leading directly to the stage. This dressing room can comfortably hold 8 people. In the dressing room there are shower and toilet facilities.

**Access**

The auditorium and bar are accessed through one door and down a flight of stairs past the box office. Disabled access is available (please phone for full details on 0207 930 2949 during office hours 11 – 6). Wheelchair positions in the auditorium are available if prior notice is given to the General Manager. There are disabled toilet facilities available in The Comedy Store London.

**Outside Venues**

If you would prefer to host an event in a venue other than The Comedy Store and are looking for comedians to perform at your event, our Artist Management service can help you.